(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "AudioJack_CUI_SJ1-3525N" (in_bom yes) (on_board yes)
    (property "Reference" "J2" (at 0.635 7.62 90)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Value" "CUI_SJ1_3525N" (at -1.905 7.62 90)
      (effects (font (size 1.27 1.27)) (justify left))
    )
    (property "Footprint" "electrosluch_parts:CUI_SJ1-3525N" (at -2.54 5.08 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 -12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Audio Jack, 3 Poles (Stereo / TRS), Switched TR Poles (Normalling)" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "Jack*" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "AudioJack_CUI_SJ1-3525N_0_1"
      (rectangle (start -5.08 -5.08) (end -6.35 -7.62)
        (stroke (width 0.254) (type default))
        (fill (type outline))
      )
      (rectangle (start -5.08 3.81) (end 2.54 -10.16)
        (stroke (width 0.254) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 0.508 -0.254)
          (xy 0.762 -0.762)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.778 -5.334)
          (xy 2.032 -5.842)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0 -5.08)
          (xy 0.635 -5.715)
          (xy 1.27 -5.08)
          (xy 2.54 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -7.62)
          (xy 1.778 -7.62)
          (xy 1.778 -5.334)
          (xy 1.524 -5.842)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 -2.54)
          (xy 0.508 -2.54)
          (xy 0.508 -0.254)
          (xy 0.254 -0.762)
        )
        (stroke (width 0) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.905 -5.08)
          (xy -1.27 -5.715)
          (xy -0.635 -5.08)
          (xy -0.635 0)
          (xy 2.54 0)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.54 2.54)
          (xy -2.54 2.54)
          (xy -2.54 -5.08)
          (xy -3.175 -5.715)
          (xy -3.81 -5.08)
        )
        (stroke (width 0.254) (type default))
        (fill (type none))
      )
    )
    (symbol "AudioJack_CUI_SJ1-3525N_1_1"
      (pin passive line (at 5.08 0 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "R" (effects (font (size 1.27 1.27))))
        (alternate "3" passive line)
      )
      (pin passive line (at 5.08 -2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "RN" (effects (font (size 1.27 1.27))))
        (alternate "11" passive line)
      )
      (pin passive line (at 5.08 2.54 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "S" (effects (font (size 1.27 1.27))))
        (alternate "1" passive line)
      )
      (pin passive line (at 5.08 -5.08 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "T" (effects (font (size 1.27 1.27))))
        (alternate "2" passive line)
      )
      (pin passive line (at 5.08 -7.62 180) (length 2.54)
        (name "~" (effects (font (size 1.27 1.27))))
        (number "TN" (effects (font (size 1.27 1.27))))
        (alternate "10" passive line)
      )
    )
  )
)
