(footprint "Jack_3.5mm_CUI_SJ1-3525N_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
  (tags "TRS audio jack stereo horizontal")
  (property "Sheetfile" "electrosluch_basic.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Audio Jack, 3 Poles (Stereo / TRS), Switched TR Poles (Normalling)")
  (property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector")
  (attr through_hole exclude_from_pos_files)
  (fp_text reference "J2" (at 6.778 -6.985 -90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 896d6f42-48b7-40c6-b9f8-788e0ec81504)
  )
  (fp_text value "AudioJack2_Ground_Switch" (at 0 -10) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6da8155b-d230-4e05-9f13-8890262446d7)
  )
  (fp_text user "PCB edge" (at 0 2.54 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8baa94ca-3573-4aaf-b79d-5a8387c8672f)
  )
  (fp_line (start -6 -7.7) (end 6 -7.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f6722ec9-9548-427e-9d54-6f5eec66c62a))
  (fp_line (start -6 3.3) (end -6 -7.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3a715105-39ca-4dd1-acd6-c1dfa00bfd5b))
  (fp_line (start -4.5 3.3) (end -6 3.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ed63ae8-ef74-4b81-8fb7-422cde8799c0))
  (fp_line (start 6 -7.7) (end 6 3.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 561143bf-3cc1-4d38-81d0-0f1fffe20d57))
  (fp_line (start 6 3.3) (end 4.5 3.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b3331f93-011e-4a61-aa65-3a813c884cc0))
  (fp_line (start -6.25 -7.95) (end -6.25 4.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4860311b-fc6b-4675-bd68-a538eb16fd9a))
  (fp_line (start -6.25 4.75) (end -3.25 4.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ab86fff8-0d29-4dac-bffe-5993f2a178f9))
  (fp_line (start -3.25 4.75) (end -3.25 6.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 62d74b4d-493a-47ef-9b70-6eb999507277))
  (fp_line (start -3.25 6.55) (end 3.25 6.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c5cb9bae-faa1-41fc-ba96-58f85722a631))
  (fp_line (start 3.25 4.75) (end 6.25 4.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8835e521-3e91-451a-8112-bb0501bac3d3))
  (fp_line (start 3.25 6.55) (end 3.25 4.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 55ffb7c0-515b-4899-94be-918a2093c62b))
  (fp_line (start 6.25 -7.95) (end -6.25 -7.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 76e05852-0321-4c8a-bd14-86717f420989))
  (fp_line (start 6.25 4.5) (end 6.25 -7.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1d4b3562-f4ef-4d89-bb5f-312b3e2e85fc))
  (fp_line (start 6.25 4.75) (end 6.25 4.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 532e636f-b4ed-471d-bdfa-1d9feb8ed8c6))
  (fp_line (start -6 -7.7) (end 6 -7.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a51bc3bf-5940-499d-b419-ca0879a09e77))
  (fp_line (start -6 3.3) (end -6 -7.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b2cdf306-a138-45a2-a167-13c27629d6b4))
  (fp_line (start -4.5 3.3) (end -6 3.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b2251fc4-7ee7-4258-afe9-2b31fc8b7325))
  (fp_line (start 4.5 3.3) (end 6 3.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp beda5cef-6364-4612-8fa1-5d772a42c21a))
  (fp_line (start 6 3.3) (end 6 -7.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fecfc4b2-99e8-400c-a6b4-a9bba4c9b553))
  (pad "" np_thru_hole circle (at -5 0) (size 1.2 1.2) (drill 1.2) (layers "*.Cu") (tstamp e6f0c64b-30ca-43b1-9bef-e7bb06679a2e))
  (pad "" np_thru_hole circle (at -5 2.5) (size 1.2 1.2) (drill 1.2) (layers "*.Cu") (tstamp 52c94bbb-f774-4a67-976e-9247d0b3d3b3))
  (pad "" np_thru_hole circle (at 0 -5) (size 1.2 1.2) (drill 1.2) (layers "*.Cu") (tstamp 7a40362d-e929-42f7-befa-106ec67eaea2))
  (pad "" np_thru_hole circle (at 0 4.191) (size 1.016 1.016) (drill oval 5.5 2) (layers "F&B.Cu") (tstamp 6dc9c6f2-8d7a-4e53-a7d7-8d51f97ba6ec))
  (pad "" np_thru_hole circle (at 5 0) (size 1.2 1.2) (drill 1.2) (layers "*.Cu") (tstamp c29b54ab-bbdd-4e88-9a71-b289ffcc9e14))
  (pad "" np_thru_hole circle (at 5 2.5) (size 1.2 1.2) (drill 1.2) (layers "*.Cu") (tstamp c5011f32-35db-45c7-aeb9-614c2f708120))
  (pad "R" thru_hole oval (at -5 -5) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask") (tstamp 092e47c5-8ea5-47c7-9a3c-1dd2a81512cc))
  (pad "RN" thru_hole oval (at -2.5 -5) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask") (tstamp fbee2740-fadc-42e3-bfc7-f53322562ce1))
  (pad "S" thru_hole oval (at 0 0) (size 2.2 1.2) (drill oval 1.4 0.4) (layers "*.Cu" "*.Mask") (tstamp 2eed4e70-4527-4a2d-9150-a58a4f55ce27))
  (pad "T" thru_hole oval (at 5 -5 180) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask") (tstamp 533bd577-d060-4586-bb01-d1b85a953050))
  (pad "TN" thru_hole oval (at 2.5 -5 180) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask") (tstamp aa895625-0051-4d99-a575-ea3cac6b12d9))
  (model "${KIPRJMOD}/SJ1-3525N.stp"
    (offset (xyz 0 -6.8 2.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
