# Cockstar

Cocktail robot to automatically dose rum for Tschunk.

![](images/cockstar.jpg)


## Hardware Configuration

### Functionality:
* 0	    off
* 1-99	amount in ml
* 100   permanent on


LED-Ring has 12 LEDs

Pumpe has 22 LEDs.


### Connect LCD:
* LCD		Arduino
* VCC		5V
* GND		GND
* SDA		A4
* SCL		A5


### Connect Poti:
* Red		A0
* Gray	5v
* Blue	GND


### Connect Switch: 
* White/Red	D12
* Black (LED)	D11

### Bottle
* White (D IN)    D10

### Connect Relay
* Input	D13	

### Connect Pump
* LED Output D9 or D11


## Software
Cockstar uses new LiquidCrystal https://bitbucket.org/fmalpartida/new-liquidcrystal/wiki/Home
